# TABLE OF CONTENTS

1. INTRODUCTION 1-1
2. PAVEMENT TYPES 2-1

Introduction **2-1**

Pavement Types **2-3**

1. PAVEMENT MATERIALS 3-1

Soil and Aggregate 3-1

Asphalt Pavement 3-20

Concrete Pavement 3-37

1. **STRUCTURAL DESIGN** 4-1

AASHTO Pavement Design Procedures 4-1

Mechanistic-Empirical Pavement Design 4-8

AASHTOWare Pavement ME Design™ 4-11

AASHTOWare Pavement ME Design™ Analysis/Design Approach 4-12

Design of New and Reconstructed Asphalt Pavements 4-36

Design of New and Reconstructed Concrete Pavements 4-39

Design of New and Reconstructed Composite Pavements 4-42

Design of Rehabilitated Pavements 4-42

Surface and Subsurface Drainage Design 4-46

**5. PAVEMENT SURFACE CHARACTERISTICS** 5-1

Pavement Smoothness or Roughness 5-2

Surface Texture 5-12

Porosity 5-25

Friction 5-26

Hydroplaning Potential 5-34

Splash/Spray 5-36

Noise 5-38

Other Dynamic Attributes 5-51

Surface Characteristics and User Costs 5-52

**6. PAVEMENT TYPE SELECTION** 6-1

Federal Policy Regarding Pavement Type Selection and LCCA 6-1

Guidance for Pavement Type Selection 6-2

Guidance for Life Cycle Cost Analysis 6-4

**7. PAVEMENT CONSTRUCTION** 7-1

Quality Management 7-1

Construction Practices for Subgrades 7-4

Construction Practices for Bases 7-12

Construction Practices for Asphalt Pavements 7-19

Construction Practices for Concrete Pavements 7-48

1. PAVEMENT EVALUATION 8-1

Pavement Distress 8-2

Pavement Distress Survey Techniques 8-5

Field Sampling and Testing 8-12

Pavement Drainage Surveys 8-18

**9. STRUCTURAL TESTING AND ANALYSIS** 9-1

Destructive Sampling and Testing 9-1

Nondestructive Testing (NDT) Techniques for Pavement Assessment 9-1

Backcalculation and Deflection Analysis 9-19

Accelerated Pavement Testing 9-26

Forensic Investigation 9-30

**10. PAVEMENT PRESERVATION TREATMENTS** 10-1

Pavement Preservation Concepts 10-1

Preventive Maintenance Treatments 10-6

Treatment/Project Selection 10-56

**11. PAVEMENT REHABILITATION STRATEGIES** 11-1

Pre Rehabilitation Treatments 11-1

Asphalt Pavement Rehabilitation Treatment Types 11-4

Concrete Pavement Rehabilitation Treatment Types 11-18

Composite Pavement Rehabilitation Treatment Types 11-49

Rehabilitation Treatment/Project Selection 11-53

**12. PAVEMENT MANAGEMENT** 12-1

Basic Pavement Management Framework 12-1

Pavement Management Components 12-1

Benefits of Using Pavement Management 12-2

Pavement Condition Assessment 12-3

Pavement Inventory Data 12-6

Pavement Performance Modeling 12-7

Project and Treatment Selection 12-9

Implementing a Pavement Management System 12-12

Future Directions in Pavement Management 12-13

Asset Management Principles 12-14

**13. PAVEMENT SUSTAINABILITY** 13-1

Sustainability Factors 13-5

General Strategies for Improving Pavement Sustainability 13-6

Sustainable Practices for Asphalt Pavements 13-8

Sustainable Practices for Concrete Pavements 13-11

Assessment of Sustainable Practices 13-15

Concluding Remarks on Pavement Sustainability 13-17

**LIST OF FIGURES**

Figure 2-1. Basic components of a typical pavement system. 2-1

Figure 2-2. Asphalt pavement structure and load distribution. 2-3

Figure 2-3. Concrete pavement structure and load distribution. 2-4

Figure 2-4. Composite pavements. 2-4

Figure 2-5. Common asphalt pavement structural designs. 2-6

Figure 2-6. Typical concrete pavement cross-section. 2-11

Figure 2-7. Concrete pavement joints. 2-12

Figure 2-8. Schematic of a JPCP pavement design. 2-13

Figure 2-9. Schematic of a JRC pavement design. 2-14

Figure 2-10. Schematic of a CRC pavement design 2-14

Figure 2-11. Pervious concrete pavement cross-section. 2-16

Figure 2-12. Continuous application of precast concrete slabs. 2-17

Figure 3-1. Semi-log plot of a sample gradation. 3-3

Figure 3-2. 0.45 power scale. 3-3

Figure 3-3. Triaxial cell for testing cylindrical specimens. 3-6

Figure 3-4. Approximate relationships between various soil classifications and properties. 3-9

Figure 3-5. Volumetric and mass relationships for a soil shown as a phase diagram. 3-10

Figure 3-6. Four moisture states of aggregate. 3-11

Figure 3-7. Typical moisture-density plot illustrating optimal moisture content. 3-12

Figure 3-8. Particle angularity. 3-14

Figure 3-9. Flat and elongated particles. 3-14

Figure 3-10. Aggregate with 100 percent non-fractured faces and aggregate with 100
percent fractured faces. 3-15

Figure 3-11. Calipers for evaluating flat and elongated particles. 3-15

Figure 3-12. Distillation of crude petroleum. 3-22

Figure 3-13. Asphalt mixture phase diagram 3-32

Figure 3-14. Superpave gradation control plot for 12.5 mm nominal maximum aggregate
size. 3-34

Figure 3-15. Superpave gyratory compactor. 3-36

Figure 3-16. Manufacturing process for portland cement 3-39

Figure 3-17. Fly ash and a scanning electron micrograph of fly ash particles. 3-44

Figure 3-18. Slag cement and a scanning electron micrograph of slag particles. 3-45

Figure 3-19. Silica fume and a scanning electron micrograph of silica fume. 3-46

Figure 3-20. Metakaolin and a scanning electron micrograph of calcined clay particles. 3-46

Figure 3-21. Ternary diagram illustrating the oxide composition of cement and common SCMs. 3-47

Figure 3-22. Diagram illustrating the particle size distribution of cement and common
SCMs. 3-48

Figure 3-23. Stereomicroscope micrograph of entrained air-void system. 3-52

Figure 3-24. Illustration of spacing factor. 3-53

Figure 3-25. Compressive strength test. 3-61

Figure 3-26. Third-point flexural testing. 3-62

Figure 3-27. Splitting tensile strength test 3-63

Figure 3-28. Durability cracking at Coles County Memorial Airport in Mattoon, IL 3-67

Figure 3-29. Example relationship between compressive strength and w/cm for concrete
using 0.75-in to 1.0-in nominal maximum size coarse aggregate. 3-72

Figure 3-30. Modified coarseness factor chart. 3-74

Figure 3-31. 0.45 power chart for 1-in nomimal maximum aggregate. 3-75

Figure 3-32. Percent aggregate retained chart. 3-75

Figure 3-33. Target total air content requirements for concrete with different aggregate
sizes. 3-76

Figure 4-1. Lateral traffic wander. 4-16

Figure 4-2. Mean wheel location. 4-16

Figure 4-3. General design methodology. 4-31

Figure 4-4. Reliability concept. 4-32

Figure 4-5. General calibration flowchart. 4-34

Figure 4-6. Critical asphalt pavement response locations. 4-37

Figure 4-7. Critical JPCP response locations. 4-40

Figure 4-8. Critical CRCP response locations. 4-40

Figure 4-9. Permeable base with edgedrain. 4-50

Figure 4-10. Headwall. 4-51

Figure 4-11. Nonerodible base with edgedrain. 4-51

Figure 4-12. Nonerodible base, edgedrain, and porous concrete shoulder. 4-52

Figure 4-13. Daylighted permeable base. 4-53

Figure 4-14. Daylighted dense-graded aggregate base. 4-53

Figure 4-15. Formation of ice lenses in a pavement structure. 4-55

Figure 5-1. Longitudinal and lateral profiles along roadway surface. 5-3

Figure 5-2. Dipstick® equipment and operation. 5-4

Figure 5-3. California Profilograph. 5-5

Figure 5-4. Schematic of profile van. 5-6

Figure 5-5. Example of profile van. 5-6

Figure 5-6. Example of pavement condition van. 5-7

Figure 5-7. Profilograph trace and PI computation. 5-10

Figure 5-8. IRI range by roadway type. 5-11

Figure 5-9. Illustration of microtexture and macrotexture of a road surface. 5-12

Figure 5-10. Illustration of microtexture, macrotexture, and megatexture for road
surfaces. 5-13

Figure 5-11. British pendulum tester. 5-14

Figure 5-12. DF Tester. 5-15

Figure 5-13. Sand patch test kit. 5-16

Figure 5-14. CT Meter. 5-16

Figure 5-15. RoboTex low-speed texture measurement system. 5-17

Figure 5-16. RoboTex three-dimensional texture plot. 5-17

Figure 5-17. High-speed texture profiling system. 5-18

Figure 5-18. Texture measurement using the OF Meter. 5-19

Figure 5-19. Pavement surface texture spectrum. 5-21

Figure 5-20. Simplified diagram of forces acting on a rotating wheel. 5-27

Figure 5-21. Pavement friction versus tire slip. 5-28

Figure 5-22. Key mechanisms of pavement–tire friction. 5-29

Figure 5-23. Locked-wheel friction trailer. 5-30

Figure 5-24. Ribbed and smooth test tires used for locked-wheel friction testing. 5-31

Figure 5-25. Example of a possible PFM program. 5-33

Figure 5-26. Weighting curves used for sound pressure level adjustment. 5-39

Figure 5-27. Example of various sound level measurements. 5-40

Figure 5-28. CPX trailer. 5-42

Figure 5-29. CPX trailer close-up. 5-42

Figure 5-30. OBSI equipment. 5-43

Figure 5-31. Acoustical absorption test equipment. 5-45

Figure 5-32. Texture measurement equipment. 5-46

Figure 5-33. OGFC surface texture. 5-46

Figure 5-34. SMA aggregate structure. 5-47

Figure 5-35. European two-layer asphalt design. 5-48

Figure 5-36. NGCS single-pass diamond grinding head. 5-49

Figure 5-37. NGCS second pass diamond grinding head. 5-49

Figure 5-38. Next generation concrete surface. 5-50

Figure 5-39. Two-lift concrete construction. 5-51

Figure 6-1. Pavement-type selection process. 6-2

Figure 6-2. Process for conducting project-level pavement LCCA. 6-4

Figure 6-3. Illustration of analysis period for a pavement design strategy. 6-5

Figure 6-4. Alternatives performance curve comparison. 6-9

Figure 6-5. Example probability distribution 6-11

Figure 6-6. Example of expenditure stream diagram 6-12

Figure 6-7. Example expenditure stream diagram for a pavement design alternative 6-13

Figure 6-8. Example tornado plot. 6-15

Figure 7-1. Finished subgrade. 7-5

Figure 7-2. Chemical stabilization of subgrade soil 7-6

Figure 7-3. Stabilized and unstabilized subgrade construction process. 7-8

Figure 7-4. Placement of thick granular layer. 7-9

Figure 7-5. Geosynthetics construction sequence. 7-11

Figure 7-6. Unstabilized base construction process. 7-14

Figure 7-7. Placement of ATB. 7-14

Figure 7-8. Cement-treated base construction. 7-17

Figure 7-9. Lean concrete base construction. 7-18

Figure 7-10. Batch plant elements. 7-21

Figure 7-11. Drum-mix plant elements. 7-22

Figure 7-12. Tack coat application. 7-25

Figure 7-13. Broken tack coat. 7-26

Figure 7-14. Example of an end-dump truck. 7-27

Figure 7-15. Example of an end-dump truck with windrow blender device. 7-27

Figure 7-16. Example of bottom-dump truck. 7-28

Figure 7-17. Example of live-bottom dump truck. 7-28

Figure 7-18. Schematic of asphalt mixture paver. 7-29

Figure 7-19. Schematic of material feed system 7-30

Figure 7-20. Example of a windrow elevator. 7-32

Figure 7-21. Examples of a surge volume/remixer. 7-32

Figure 7-22. Safety Edge for asphalt pavements and asphalt overlays. 7-33

Figure 7-23. Example of an asphalt pavement Safety Edge. 7-34

Figure 7-24. Example of paver screed. 7-35

Figure 7-25. Example of steel wheel roller. 7-36

Figure 7-26. Example of steel wheel finish roller. 7-36

Figure 7-27. Example of pneumatic tire roller. 7-37

Figure 7-28. Poorly performing longitudinal joints. 7-39

Figure 7-29. Offset multiple lifts of asphalt mixture. 7-39

Figure 7-30. Proper construction of first paver pass. 7-40

Figure 7-31. Compaction of the unsupported edge. 7-40

Figure 7-32. Compaction of the confined edge. 7-41

Figure 7-33. Example of image showing temperature-density differentials. 7-42

Figure 7-34. Dry concrete batch plant. 7-49

Figure 7-35. Wet (or central mix) concrete batch plant. 7-49

Figure 7-36. Concrete paving methods. 7-51

Figure 7-37. Slipform concrete placement. 7-52

Figure 7-38. Components of a slipform paver. 7-52

Figure 7-39. Example of fixed form concrete placement. 7-53

Figure 7-40. String line for concrete placement. 7-54

Figure 7-41. Dowel bar baskets and dowel bar inserter. 7-56

Figure 7-42. Tie bar baskets and tie bar inserter. 7-56

Figure 7-43. Use of bull floats to remove minor surface irregularities. 7-57

Figure 7-44. Transverse construction joint. 7-58

Figure 7-45. Example of drag texturing. 7-59

Figure 7-46. Longitudinal tining. 7-59

Figure 7-47. Applying curing compound. 7-61

Figure 7-48. Safety Edge for concrete pavements and concrete overlays. 7-64

Figure 7-49. Example of Safety Edge. 7-65

Figure 8-1. Types of distress data collected. 8-5

Figure 8-2. Steps in data collection and analysis 8-8

Figure 8-3. Example of a sampling approach. 8-11

Figure 8-4. Schematic diagram of FWD testing equipment. 8-16

Figure 9-1. Typical pavement deflection basin. 9-2

Figure 9-2. Benkelman Beam. 9-3

Figure 9-3. Dynaflect. 9-3

Figure 9-4. Example of FWD. 9-4

Figure 9-5. Air-coupled GPR. 9-7

Figure 9-6. GPR principles. 9-8

Figure 9-7. GPR scan of CRCP. 9-9

Figure 9-8. UPV testing. 9-10

Figure 9-9. Schematic of impact echo. 9-12

Figure 9-10. Schematic of SASW. 9-14

Figure 9-11. PSPA. 9-15

Figure 9-12. MIT Scan T2. 9-16

Figure 9-13. Placement of metal reflector prior to paving. 9-17

Figure 9-14. Pachometer schematic. 9-18

Figure 9-15. MIT Scan-2 being used for measuring dowel. 9-19

Figure 9-16. Depiction of load transfer. 9-24

Figure 9-17. Example void detection plot. 9-25

Figure 9-18. ATLAS test facility. 9-26

Figure 9-19. Florida HVS mobile testing device. 9-27

Figure 9-20. Caltrans HVS mobile testing device. 9-27

Figure 9-21. NCAT pavement test track. 9-28

Figure 9-22. MnROAD test road 9-29

Figure 10-1. Relationship between pavement condition and different categories of
pavement treatment. 10-2

Figure 10-2. Typical pavement condition as a function of time. 10-4

Figure 10-3. Crack sealing/filling. 10-8

Figure 10-4. Examples of crack refacing equipment. 10-10

Figure 10-5. Examples of crack cleaning and drying equipment. 10-11

Figure 10-6. Sealant configurations. 10-11

Figure 10-7. Example of sealant placement and shaping. 10-12

Figure 10-8. Placement of blotter sand. 10-12

Figure 10-9. Fog seal application. 10-13

Figure 10-10. Fog seal/rejuvenator application. 10-15

Figure 10-11. Slurry seal and microsurfacing applications. 10-16

Figure 10-12. Examples of slurry seal/microsurfacing spreader boxes. 10-18

Figure 10-13. Chip seal application. 10-18

Figure 10-14. Chip seal aggregate application. 10-20

Figure 10-15. Rolling aggregate for chip seal application. 10-21

Figure 10-16. Thin asphalt application. 10-22

Figure 10-17. Ultra-thin bonded wearing course. 10-24

Figure 10-18. Example of special paving equipment for ultra-thin bonded wearing
course. 10-26

Figure 10-19. HIR recycling train. 10-27

Figure 10-20. Example of HIR heater scarifier unit. 10-29

Figure 10-21. Example of HIR scarifier. 10-29

Figure 10-22. Example of HIR mixing unit. 10-30

Figure 10-23. Joint resealing. 10-33

Figure 10-24. Diamond grinding. 10-35

Figure 10-25. Diamond grinding head. 10-35

Figure 10-26. Dowel bar retrofit. 10-37

Figure 10-27. Slot cutting equipment. 10-38

Figure 10-28. Removing existing concrete material between sawcuts. 10-39

Figure 10-29. Cleaning the dowel bar retrofit slot. 10-39

Figure 10-30. Caulking existing joints or cracks within the dowel bar retrofit slot. 10-40

Figure 10-31. Dowel bar assemblies inserted into the dowel bar slots. 10-40

Figure 10-32. Placing grout material into dowel bar retrofit slot. 10-41

Figure 10-33. Drilling injection hole for subsealing. 10-42

Figure 10-34. Recommended subsealing injection hole pattern. 10-43

Figure 10-. Slab replacement 10-44

Figure 10-. Spall repair 10-45

Figure 10-37. Repair boundary recommendations for JPCP. 10-47

Figure 10-38. Repair boundary recommendations for JRCP. 10-47

Figure 10-39. Repair boundary recommendations for CRCP. 10-48

Figure 10-40. Example of relief cuts for full-depth slab repair. 10-49

Figure 10-41. Recommended sawcuts for CRCP. 10-50

Figure 10-42. Concrete removal using breakup method. 10-50

Figure 10-43. Concrete removal using lift-out method. 10-51

Figure 10-44. Repair area preparation. 10-51

Figure 10-45. Recommended dowel bar placement 10-52

Figure 10-46. Welded or mechanical connection details for CRCP repairs 10-52

Figure 10-47. Placing concrete for full-depth repair. 10-53

Figure 10-48. Texturing concrete for full-depth repair. 10-53

Figure 10-49. Applying curing compound for full-depth repair. 10-54

Figure 10-50. Sawcutting spall repair boundary. 10-55

Figure 10-51. Compressible insert for spall repair. 10-55

Figure 11-. HMA milling 11-2

Figure 11-. Milled surface 11-3

Figure 11-3. Asphalt overlay application. 11-4

Figure 11-4. Plant with RAP in feed. 11-8

Figure 11-5. Asphalt cold central plant recycling. 11-10

Figure 11-6. Cold in-place recycling. 11-10

Figure 11-7. Full-depth reclamation schematic. 11-11

Figure 11-8. Full-depth reclaiming. 11-12

Figure 11-9. Bonded concrete overlay of existing asphalt. 11-14

Figure 11-10. Unbonded concrete overlay of existing asphalt pavement 11-17

Figure 11-11. Transverse sawcut for unbonded concrete overlays. 11-18

Figure 11-12. Bonded concrete overlay of existing concrete pavement. 11-19

Figure 11-13. Unbonded concrete overlay of existing concrete pavement. 11-22

Figure 11-14. Guillotine hammer. 11-29

Figure 11-15. Impact hammer. 11-30

Figure 11-16. Resonant breaker. 11-34

Figure 11-17. Resonant breaker surface. 11-34

Figure 11-18. Multi-head breaker. 11-35

Figure 11-19. Multi-head breaker surface. 11-35

Figure 11-20. Compact rubblized layer using a 11-grid roller. 11-37

Figure 11-21. Compacted rubblized concrete surface. 11-37

Figure 11-22. Recycled concrete aggregate. 11-38

Figure 11-23. Bonded concrete overlay of an existing composite pavement. 11-49

Figure 11-24. Unbonded concrete overlay of existing concrete pavement. 11-51

Figure 11-25. Example decision trees for rehabilitation and preventive maintenance. 11-60

Figure 11-26. Decision tree for rehabilitation of JPCP. 11-61

Figure 12-1. Pavement management components. 12-2

Figure 12-2. Backlog and PCI over time and under different annual funding scenarios. 12-11

Figure 12-3. Steps in establishing a performance management program. 12-15

Figure 12-4. Concept for an asset management analytical toolbox. 12-16

Figure 12-5. Asset management implementation steps. 12-17

Figure 13-1. Graphical representation of sustainability’s “triple-bottom line” of economic, environmental, and societal interests. 13-2

Figure 13-2. The pavement life cycle. 13-3

Figure 13-3. INVEST credit comparison chart including which triple-bottom line
principles are addressed by each credit. 13-18

**LIST OF TABLES**

Table 3-1. Common sieve designations and sizes used in highway construction. 3-2

Table 3-2. Subgrade soil types and approximate k values 3-7

Table 3-3. AASHTO Soil Classification. 3-17

Table 3-4. USCS Classification. 3-18

Table 3-5. AASHTO coarse aggregate gradations. 3-19

Table 3-6. Performance graded asphalt binder specification. 3-23

Table 3-7. Binder grades in the performance-graded asphalt binder specifications. 3-24

Table 3-8. Grades of asphalt emulsions. 3-25

Table 3-9. Recommended Superpave aggregate consensus properties. 3-34

Table 3-10. Nominal maximum aggregate size by application 3-35

Table 3-11. High temperature grade adjustments by traffic level and speed 3-35

Table 3-12. Ndesign at specific design traffic levels. 3-36

Table 3-13. VMA targets by nominal maximum aggregate size 3-37

Table 3-14. Applications for hydraulic cements. 3-38

Table 3-15. Summary of effects of SCMs on the fresh and hardened properties of
concrete 3-48

Table 3-16. Concrete admixtures for concrete by classification 3-51

Table 3-17. Recommended air contents for concrete resistant to freezing and thawing 3-68

Table 3-18. Requirements to protect against damage to concrete by sulfate attack from external sources of sulfate 3-70

Table 3-19. Maximum w/cm and minimum design strengths for various exposure
conditions 3-72

Table 3-20. Types of cement and minimum w/cm requirements for concrete exposed to sulfates in soil and water 3-73

Table 3-21. Recommended cementitious materials for concrete exposed to deicing
chemicals 3-77

Table 3-22. Suggested laboratory testing plan for trial batches 3-80

Table 3-23. Suggested field trial batch testing plan 3-81

Table 4-1. AASHO Road Test climatic conditions. 4-2

Table 4-2. AASHO Road Test traffic loads. 4-2

Table 4-3. AASHO Road Test asphalt pavement details. 4-2

Table 4-4. AASHO Road Test concrete pavement details. 4-3

Table 4-5. Traffic data requirements by input level. 4-14

Table 4-6. Estimating new asphalt layer parameters. 4-18

Table 4-7. Estimating concrete layer parameters. 4-21

Table 4-8. Recommended overall condition assessment of the existing concrete layer. 4-23

Table 4-9. Recommended concrete pavement condition factor. 4-24

Table 4-10. Recommended modulus range based on concrete pavement condition factor. 4-25

Table 4-11. Recommended modulus range for fractured concrete slabs. 4-25

Table 4-12. Estimating stabilized layer parameters. 4-25

Table 4-13. Characterizing unbound layer and subgrade inputs. 4-27

Table 4-14. Recommended reliability levels by functional class. 4-33

Table 4-15. Recommended minimum sample size. 4-35

Table 4-16. Pavement evaluation by hierarchical level. 4-43

Table 4-17. Summary of inputs for asphalt rehabilitation. 4-44

Table 4-18. Summary of inputs for concrete rehabilitation. 4-45

Table 4-19. Summary of rehabilitation inputs for chemically stabilized layers. 4-46

Table 4-20. Summary of rehabilitation inputs for soil and unbound layers. 4-47

Table 4-21. Material characteristics of permeable bases. 4-49

Table 4-22. Frost susceptibility by soil classification. 4-54

Table 5-1. Effects of physical attributes on dynamic attributes. 5-1

Table 5-2. Effects of dynamic attributes on the highway users. 5-2

Table 5-3. Summary of roughness measurement equipment. 5-8

Table 5-4. Construction considerations for macrotexture in asphalt-surfaced
pavements. 5-23

Table 5-5. Construction considerations for macrotexture in concrete pavements. 5-24

Table 5-6. Assessment of hydroplaning potential based on vehicle speed and water film thickness. 5-35

Table 5-7. Common activity noise levels. 5-39

Table 6-1. Recent trends in real discount rates 6-7

Table 7-1. Subgrade soil conditions and stabilization methods. 7-10

Table 7-2. Recommended material specifications for ATB. 7-15

Table 7-3. Recommended material specifications for CTB/LCB. 7-16

Table 7-4. Recommended tack coat rates. 7-24

Table 7-5. Asphalt pavement smoothness checklist. 7-45

Table 7-6. Quality control tests for concrete pavements. 7-69

Table 7-7. Concrete pavement smoothness checklist 7-71

Table 8-1. Pavement distresses. 8-3

Table 8-2. Pavement distresses identified for PCI. 8-4

Table 8-3. Advantages and disadvantages of manual surveys. 8-6

Table 8-4. Advantages and disadvantages of automated surveys. 8-8

Table 9-1. Summary of deflection testing recommendations. 9-5

Table 9-2. Deflection testing summary. 9-5

Table 9-3. GPR accuracy by pavement type. 9-9

Table 9-4. GPR testing summary. 9-10

Table 9-5. UPV testing summary. 9-11

Table 9-6. Impact echo testing summary. 9-13

Table 9-7. SASW testing summary. 9-14

Table 9-8. PSPA testing summary. 9-15

Table 9-9. Pachometer testing summary. 9-18

Table 9-10. MIT Scan-2 testing summary. 9-19

Table 9-11. Available backcalculation programs. 9-20

Table 9-12. Addressing specific conditions in pavement backcalculation analysis 9-21

Table 10-1. Crack sealing versus crack filling. 10-8

Table 10-2. Key characteristics of crack sealing/filling. 10-9

Table 10-3. Guidelines for crack sealing/filling. 10-10

Table 10-4. Key characteristics of fog seals/rejuvenators. 10-14

Table 10-5. Fog seals/rejuvenators design features. 10-15

Table 10-6. Key characteristics of slurry seals/microsurfacing. 10-17

Table 10-7. Key characteristics of chip seals. 10-19

Table 10-8. Key characteristics of thin asphalt overlays. 10-23

Table 10-9. Key characteristics of ultra-thin bonded wearing course. 10-25

Table 10-10. Key characteristics of hot in-place recycling. 10-28

Table 10-11. Key characteristics of in-place recycling. 10-31

Table 10-12. CIR equipment summary. 10-32

Table 10-13. Key characteristics of crack sealing/joint resealing. 10-34

Table 10-14. Key characteristics of diamond grinding. 10-36

Table 10-15. Key characteristics of load transfer restoration. 10-38

Table 10-16. Key characteristics of undersealing. 10-42

Table 10-17. Key characteristics of concrete pavement patching. 10-46

Table 10-18. Examples of high early-strength mix designs and approximate opening
times. 10-49

Table 10-19. Key characteristics of drainage preservation. 10-57

Table 11-1. Typical maximum joint spacing for unbonded concrete overlay of concrete pavement. 11-24

Table 11-2. Comparison of typical virgin aggregate and RCA properties. 11-41

Table 11-3. Typical specifications for coarse aggregate gradation. 11-43

Table 11-4. Properties of hardened concrete using RCA. 11-45

Table 11-5. Contaminants in concrete pavement rubble. 11-48

Table 11-6. Example candidate repair and preventive methods for distresses in asphalt pavements. 11-56

Table 11-7. Candidate repair and preventive methods for distresses in concrete
pavements. 11-57

Table 11-8. Example rehabilitation alternatives for existing asphalt pavements. 11-58

Table 11-9. Various rehabilitation alternatives for existing concrete pavements. 11-59

Table 11-10. Example worksheet of a selection process incorporating multiple selected decision factors and assigned weightings. 11-64

Table 12-1. Strategic-, network-, and project-level decisions. 12-1

Table 12-2. Distress included in the FHWA *Distress Identification Manual*. 12-4

Table 12-3. Pavement distresses identified in ASTM D6433. 12-5

Table 12-4. Pavement activities by purpose. 12-10

Table 13-1. The four certification levels within GreenroadsTM. 13-16